*Inboard Racing Commission*

**Jersey Speed Skiff**

**SAFETY INSPECTION Revised**- May 2018

# 

Boat Number

Class

Boat Name

Driver Helmet: Type Rider Helmet: Type

Snell # Snell #

C o l o r C o l o r

Driver Capsule Jacket: Category B Rider Capsule Jacket: Category B Sling: Rating in Pounds/Leg

# Of Legs

Pull Test Date (3 Yr. Max)

Driver Restraint Belts: Material: ( ) Nylon ( ) Poly Width

Release: ( ) Le v e r ( ) R o t a r y

Condition:\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Safety Cage Certification# (must be permanently mounted in boat) (Yes) (No )

## Hull

( ) 4th Forward Bulkhead & Foam - (minimum of 14” high from floor and 30” back from bow stem with this area filled completely with 2 pound density marine flotation foam) – as of June 01, 2010

( ) Steering

( ) Rudder and Bracket ( ) Strut

( ) Sling Attachment Lift Points – Accessible for viewing ( ) Motor Mounts

( ) Battery Mounts

( ) Engine Shut Off Switch (accessible to both driver & riders reach while harnessed in their seats) ( ) Propshaft Collars (2 screw or Split)

( ) Fuel tank mounts ( ) Fuel Lines

## Safety Cage

( ) Minimum 2” Clearance Above Driver/Riding Mechanic to Cage bars ( ) Attachment Points

## Trailer

( ) Trailer Numbers

( ) Fire Extinguisher (minimum 3A30BC rating) Date (5 year max)

### Inspector Event

Boat Rep Date