# 2.5 Modified Inspection Sheet – Complete inspection

Regatta: Date: Boat #

* **Length**: (Min: 16 / 166 engine alky/gas) Weight: (1325 lbs.)
* **Length**: (Min: 16’ / 155 engine alky/gas) Weight: (1225 lbs.)
* **Length**: (Min: 16’ /148.5 gasoline engine) Weight: (1025 lbs.)
* **Length**: (Min: 16’ /148.5 alky engine Weight: (1125 lbs.)

# Fuel Type (Brand name i.e. VP-C12. Methanol etc.)

# Gasoline

* + Specific Gravity (less than 0.800 @68ºF)
  + Digatron Reading (Must be negative)
* **Methanol**
  + Specific Gravity (less than 0.800 @68ºF)
* **Displacement**

Cubic Inches Measured\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ OR

Cubic Inches P&G as allowed\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* **166” and 155” Engine Options**

Two valves per cylinder only, pushrod or single overhead cam only. Methanol, Gasoline or Ethanol Fuels allowed.

* **148.5” Engine Options**

Single or Multiple Overhead Camshafts, 2 or more valves per cylinder. Gasoline or Methanol determine weight.

* **Note: A legal 2.5 stock hull may be used with the 148.5” engine combination with GASOLINE ONLY**

Chief Inspector\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ APBA # \_\_\_\_\_\_\_\_\_

Inspector\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_APBA # \_\_\_\_\_\_\_\_\_\_\_

Referee \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_APBA# \_\_\_\_\_\_\_\_\_

Inboard Commissioner \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ APBA# \_\_\_\_\_\_\_\_\_

Boat Owner’s signature\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ APBA# \_\_\_\_\_\_\_\_\_