2019 OPC Inspectors Test

Sources:

2018 General Safety & Racing Rules

2018 OPC racing Rules

Current OPC Specification Sheets

1. When an appeal is made of a technical inspection the entire engine inspection must be completed. True\_\_\_\_\_\_\_\_False\_\_\_\_\_\_\_\_
2. The SST45 Skeg Z1 minimum measurement is 3.750”. True\_\_\_\_\_\_\_False\_\_\_\_\_\_\_\_
3. Helmets bearing the Snell 2010 sticker are legal for the 2019 season. True\_\_\_False\_\_\_
4. Stock “fishing” connecting rods are illegal in SST45. True\_\_\_\_\_\_ False\_\_\_\_\_\_\_\_\_
5. Spark Advance linkage modifications are allowed in Stock and Super Stock classes. True\_\_\_\_\_False\_\_\_\_\_\_
6. Image recording cameras attached to crash helmets are not allowed. True\_\_\_\_\_\_False\_\_\_\_\_\_
7. Rules recommend that all classes with reinforced capsules/cockpits have a form fitted seat with lumbar support. True\_\_\_\_\_ False\_\_\_\_\_\_
8. Upper 50% of helmets must be a single approved color (Orange, international Orange, Yellow, Fluorescent Yellow, lime Green). True \_\_\_\_\_\_\_False\_\_\_\_\_\_\_\_\_
9. SST120 Transfer port timing is plus or minus 2̊ degrees. True\_\_\_\_\_\_False\_\_\_\_\_\_
10. At any SST200 event the referee can request trading ECU’s with other competitors. True\_\_\_\_\_\_\_False\_\_\_\_\_\_

Return completed test to:

Ken Scoville 604 Bow Mountain Road Boulder, CO 80304

303-440-0854 [ken@boatwrx.com](mailto:ken@boatwrx.com)

Include:

Name\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_APBA #\_\_\_\_\_\_\_\_\_\_

Address\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_City\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_State\_\_ Phone\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Cell\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ e-mail\_\_\_\_\_\_\_\_\_\_\_\_\_