Sportsman Advanced (SA) Technical Inspection sheet

SA (Sportsman Advanced) Class is open to all hulls, capsule or non-capsule (open boats) that meet all the current APBA runabout hull rules (Appendix A) with a maximum speed of 105 MPH (with no tolerances). The 105 MPH maximum speed will be monitored with a GPS unit in each boat. Maximum speed at time of inspection is \_\_\_\_\_\_.

Is the GPS mounted out of reach of the driver? Yes \_\_\_\_\_\_ No \_\_\_\_\_\_\_

Minimum weight, including driver and safety equipment, will be 1900 lbs. Actual weight is \_\_\_\_\_\_\_.

Does the fuel register a negative number when measured with a Digitron fuel tester? Yes \_\_\_\_ No \_\_\_\_\_ What is the number? \_\_\_\_\_\_\_.

Chief Inspector\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ APBA # \_\_\_\_\_\_\_\_\_

Inspector\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_APBA # \_\_\_\_\_\_\_\_\_\_\_

Referee \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_APBA# \_\_\_\_\_\_\_\_\_

Inboard Commissioner \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ APBA# \_\_\_\_\_\_\_\_\_

Boat Owner’s signature\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ APBA# \_\_\_\_\_\_\_\_\_