*Inboard Racing Commission*

**HYDROPLANE**

**SAFETY INSPECTION** Revised 4/18

**To Be Completed by Contestant:**

**Boat** Number Class \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Boat Name

**Driver Helmet:** Type \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Snell # \_\_\_\_\_\_\_\_\_\_\_\_\_ Color

**Life Jacket:** Category B C ( ) Flotation Vest ( ) Sewn in Uniform

**Sling:** Rating in Pounds/Leg \_\_\_\_\_\_\_\_\_\_\_\_\_\_ # Of Legs \_\_\_\_\_\_\_\_\_\_\_\_\_ Pull Test Date (3 Yr. Max)

**Driver Restraint Belts:**  Material: ( ) Nylon ( ) Poly Width \_\_\_\_\_ Release: ( ) Lever ( ) Rotary Expiration Date:

**Flotation required:** Type \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Location

**Reinforced Cockpit Certification#** (must be permanently in boat) (Yes) (No )

**To Be Completed By Inspector:**

**Hull**

( ) Steering – Cables & Puleys ( ) Rudder and Bracket

( ) Skid Fin and Mounting ( ) Strut

( ) Sling Attachment Lift Points – Accessible for viewing

( ) Motor Mounts

( ) Battery Mounts

( ) Propshaft Collars (2 screw or Split)

( ) Fuel tank mounting - where \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

( ) Fuel Lines

( ) Throttle Return Spring

( ) Mirrors

( ) Cockpit Padding

**Reinforced Cockpits**

( ) Minimum 2” Clearance Above Driver to Cockpit or Canopy

( ) The Top of the Front of the Cockpit will be a Max. of 4” Below Eye Level

( ) Minimum ½” (9 lb) Ethofoam Support Behind Head(s)

( ) No Sharp Edges or Protrusions in Cockpit

( ) Energy Absorbing Foam Padding inside Cockpit

( ) Cockpit Area Sealed (Firewall)

( ) Rollover Lift Bracket on both Sponsons (3/4” Min. Hole)

( ) Critical Information on Bottom (3” Letters) ( )Boat Number ( )Rotary ( )Air ( )Head Restraint

( ) Canopies Positive Air Flow

( ) Canopies Internal and External Release ( ) Hand Hold Opening

( ) Escape Hatch (Yes) (No)

( ) Fire Proof Driver’s Suit (Restraint Boats Only)

**Trailer**

( ) Trailer Numbers

( ) Fire Extinguisher (minimum 3A30BC rating) Date (5 year max)

Inspector \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Boat Rep

Event \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date